Eurorack Bus CV and Gate

Some of my modules take advantage of the CV and gate lines that are available in the 16-pin Eurorack power cable, to eliminate some of the patching spaghetti that doesn’t change for most of my patches. Modules that have either a gate input or a volt-per-octave pitch input will take the signal from the Eurorack bus when that input is unpatched.